|  |  |
| --- | --- |
| Date |  |
| Location |  |
| Completed by |  |

| OK = Satisfactory | AN = Action Needed | N/A = Not Applicable | **OK** | **AN** | **N/A** |
| --- | --- | --- | --- |
| 1 | Moving chains and gears are properly guarded. |[ ] [ ] [ ]
| 2 | The operator and workers in the machine area are protected from hazards created at the point of operation, ingoing nip points, rotating parts, flying chips, and sparks. |[ ] [ ] [ ]
| 3 | Operators use special hand tools for placing and removing material where needed to protect their hands. |[ ] [ ] [ ]
| 4 | Machine guards are secured and arranged so they do not cause a hazard while in use. |[ ] [ ] [ ]
| 5 | Revolving drums, barrels, and containers are guarded by an enclosure that is interlocked with the drive mechanism so that revolution cannot occur unless the guard enclosure is in place. |[ ] [ ] [ ]
| 6 | Fan blades are protected with a guard having openings no larger than 1/2" when operating within 7’ of the floor or working level. |[ ] [ ] [ ]
| 7 | Pulleys and belts within 7’ of the floor or working level are properly guarded. |[ ] [ ] [ ]
| 8 | Workers are trained on safe methods of machine operation. |[ ] [ ] [ ]
| 9 | A program is in place for regular safety inspections of machinery and equipment. |[ ] [ ] [ ]
| 10 | All machinery and equipment is kept clean and properly maintained. |[ ] [ ] [ ]
| 11 | A power shut-off switch is provided within reach of the operator’s position at each machine. |[ ] [ ] [ ]
| 12 | Hazardous energy to machines and equipment can be locked out for servicing and maintenance. |[ ] [ ] [ ]
| 13 | Foot-operated switches are guarded or arranged to prevent accidental actuation by a person or falling object. |[ ] [ ] [ ]
| 14 | Emergency stop buttons are colored red. |[ ] [ ] [ ]
| 15 | Splash guards are mounted on machines that use coolant to prevent the coolant from reaching workers. |[ ] [ ] [ ]
| 16 | Provisions are made to prevent machines from automatically starting when power is restored after a power failure or shutdown. |[ ] [ ] [ ]
| 17 | Radial arm saws are arranged so that the cutting head gently returns to the back of the table when released. |[ ] [ ] [ ]
| 18 | Abrasive grinders have safety guards that cover the spindle, nut, and flange projections; the guards are mounted to maintain proper alignment with the wheel; and the strength of the fastenings exceed the strength of the guards. |[ ] [ ] [ ]
| 19 | The adjustable tongue on the top side of the grinder is used and kept adjusted to within 1/4” of the wheel. |[ ] [ ] [ ]
| 20 | Vertical or Right Angle Head portable grinder safety guards are located between the operator and wheel during use, and have a maximum exposure angle of 180 degrees. |[ ] [ ] [ ]

|  |
| --- |
| Action Needed Items and Additional Notes: |
|  |

*This document may not be comprehensive for the requirements of the workforce or facility being evaluated. Weeklysafety.com does not assume liability for damage or injury presumed to be caused by use of this document. Use of this document does not guarantee conformity with any laws or regulations, nor does it ensure absolute workplace safety.*