|  |  |
| --- | --- |
| Date |  |
| Location |  |
| Completed by |  |

| OK = Satisfactory | AN = Action Needed | N/A = Not Applicable | **OK** | **AN** | **N/A** |
| --- | --- | --- | --- |
| Hazards that require the use of personal protective equipment (PPE) have been identified. |  |  |  |
| For all hazards identified, the appropriate and properly fitted PPE has been selected to provide suitable protection. |  |  |  |
| Affected workers use the appropriate PPE. |  |  |  |
| PPE is provided by the employer, at no cost to employees, except as noted in OSHA Standards 1910.132(h) for General Industry and 1926.95(d) for Construction. |  |  |  |
| Workers have been trained on PPE procedures, including what PPE is necessary for job tasks, when it is needed, and how to properly wear and adjust it. |  |  |  |
| Appropriate eye or face protection is used when workers are exposed to hazards such as flying particles, molten metal, liquid chemicals, acids or caustic liquids, chemical gases or vapors, or potentially injurious light radiation. |  |  |  |
| Workers who wear corrective lenses (glasses or contacts) and work in an area with potentially harmful exposures, wear eye protection that incorporates the vision prescription in the design, or wears eye protection that fits properly over their prescription lenses. |  |  |  |
| Protective eye and face protection comply with the requirements of the appropriate ANSI standards or provide protection that is at least as effective as the comparable ANSI standard. |  |  |  |
| Protective gloves, aprons, shields, or other protective equipment is used when workers could be cut or where there is a potential for exposure to corrosive liquids, chemicals, bloodborne pathogens, or other potentially infectious materials. |  |  |  |
| Hard hats are worn where the danger of falling objects exist and in any other location where there is a head protection requirement as set by the work site. |  |  |  |
| Hard hats are periodically inspected for damage and replaced if necessary. |  |  |  |
| Appropriate foot protection is worn where there is the risk of foot injuries from hot, corrosive, or poisonous substances, falling objects, crushing dangers, or penetrating actions. |  |  |  |
| Hearing protection against the effects of occupational noise is used when sound levels exceed those as outlined in OSHA Standard 1910.95 for General Industry and 1926.52 for Construction. |  |  |  |
| PPE is maintained in a safe and sanitary condition and ready for use when needed. |  |  |  |
| Appropriate procedures are in place to dispose of and replace damaged, worn, or otherwise unsafe PPE. |  |  |  |
| Appropriate procedures are in place to dispose of or decontaminate PPE that has been contaminated with (or potentially contaminated with) blood or other potentially infectious materials. |  |  |  |

|  |
| --- |
| Action Needed Items and Additional Notes: |
|  |

*This document may not be comprehensive for the requirements of the workforce or facility being evaluated. Weeklysafety.com does not assume liability for damage or injury presumed to be caused by use of this document. Use of this document does not guarantee conformity with any laws or regulations, nor does it ensure absolute workplace safety.*