|  |  |
| --- | --- |
| Date |  |
| Location |  |
| Completed by |  |

| OK = Satisfactory | AN = Action Needed | N/A = Not Applicable | **OK** | **AN** | **N/A** |
| --- | --- | --- | --- |
| 1 | The jobsite has been evaluated and permit-required confined spaces (PRCS) have been identified. |[ ] [ ] [ ]
| 2 | Danger signs are posted, or other equally effective means of informing workers is provided regarding the existence and location of, and the dangers posed by, confined spaces. |[ ] [ ] [ ]
| 3 | A written permit-required confined space program has been implemented. |[ ] [ ] [ ]
| 4 | A confined space entry permit has been completed by a qualified PRCS supervisor and posted at the entry point before entry is made. |[ ] [ ] [ ]
| 5 | Adequate illumination is provided for the work to be performed in the confined space. |[ ] [ ] [ ]
| 6 | All lines to a confined space that contain inert, toxic, flammable, or corrosive materials are valved off and blanked, or disconnected and separated before entry. |[ ] [ ] [ ]
| 7 | All sources of mechanical energy, including impellers, agitators, or other moving parts and equipment inside confined spaces, are locked out if they present a hazard. |[ ] [ ] [ ]
| 8 | All portable electrical equipment used inside confined spaces is either grounded and insulated or equipped with ground fault protection. |[ ] [ ] [ ]
| 9 | Before entry, confined spaces are thoroughly emptied of any decaying vegetation or animal matter that may produce methane or create an oxygen-deficient atmosphere. |[ ] [ ] [ ]
| 10 | Appropriate atmospheric tests are performed to check for oxygen deficiency, flammable gases, and vapors, and for potential toxic air contaminants in the confined space before entry. |[ ] [ ] [ ]
| 11 | The confined space is checked for possible industrial waste that could contain toxic properties. |[ ] [ ] [ ]
| 12 | Adequate ventilation is provided to the confined space before and during entry. |[ ] [ ] [ ]
| 13 | The atmosphere inside the confined space is frequently tested or continuously monitored during work. |[ ] [ ] [ ]
| 14 | When workers are using oxygen-consuming equipment in a confined space, sufficient air is provided to assure combustion without reducing the oxygen concentration of the atmosphere below 19.5% by volume. |[ ] [ ] [ ]
| 15 | When combustion-type equipment is used in a confined space, provisions are made to ensure exhaust gases are vented outside enclosure. |[ ] [ ] [ ]
| 16 | If the confined space is below ground and near areas where motor vehicles operate, steps are taken to prevent vehicle exhaust or carbon monoxide entering the space. |[ ] [ ] [ ]
| 17 | Approved respiratory equipment is used if the atmosphere inside the confined space cannot be made acceptable. |[ ] [ ] [ ]
| 18 | A trained attendant is positioned outside the confined space, whose sole responsibility is to watch the work in progress, sound an alarm if necessary, and render assistance. |[ ] [ ] [ ]
| 19 | The attendant has the authority to shut down the job if needed. |[ ] [ ] [ ]
| 20 | Operable communications between the entrant(s) and the attendant is maintained while workers are in the confined space. |[ ] [ ] [ ]
| 21 | Assigned attendants, entrants, and supervisors are appropriately trained and equipped to handle an emergency. |[ ] [ ] [ ]
| 22 | A means for quick removal of workers is provided, in case of an emergency. Rescuers and retrieval equipment are ready for rapid use. |[ ] [ ] [ ]
| 23 | In an emergency, the rescue workers have lifelines, retrieval equipment, and appropriate PPE including respiratory protection. |[ ] [ ] [ ]
| 24 | Before entry, operable communications with and availability of rescue services are verified. |[ ] [ ] [ ]
| 25 | Compressed gas cylinders are prohibited inside confined spaces. |[ ] [ ] [ ]
| 26 | If a hot work permit is required, it is prepared before work begins. |[ ] [ ] [ ]
| 27 | Before gas welding or burning is started in a confined space, hoses are checked for leaks, torches are lighted only outside the confined space, and the confined space is tested for an explosive atmosphere each time before a lighted torch is taken into the confined space. |[ ] [ ] [ ]
| 28 | If a new permit is required, the confined space is re-evaluated and tested before entry. |[ ] [ ] [ ]
| 29 | There is a procedure in place to ensure the safety of contract employees working in a confined space. |[ ] [ ] [ ]

|  |
| --- |
| Action Needed Items and Additional Notes: |
|  |

*This document may not be comprehensive for the requirements of the workforce or facility being evaluated. Weeklysafety.com does not assume liability for damage or injury presumed to be caused by use of this document. Use of this document does not guarantee conformity with any laws or regulations, nor does it ensure absolute workplace safety.*