| SAFETY MEETING QUIZ |
| --- |
| | Name: |  | Date: |  | | --- | --- | --- | --- | | Safety Topic: | *V1-109 Fall Protection – Suspended Scaffolds* | | | |

1. According to OSHA, suspension scaffolds, also known as swing-stage scaffolds, are perhaps the most common type of suspended scaffold.
   1. two-point adjustable
   2. three-point fixed
   3. four-point versatile
   4. five-point stationary
2. Suspension scaffold outrigger beams, cornice hooks, parapet clamps and similar devices must rest of surfaces capable of supporting at least times the load imposed on them by the scaffold, operating at the rated load of the hoist.
   1. 2
   2. 4
   3. 8
   4. 16
3. Items or material that cannot be used as counterweights include
   1. masonry units.
   2. sand or gravel.
   3. roofing felt.
   4. all of the above.
4. The scaffold platform must be at least inches wide but no more than 36 inches wide.
   1. 6
   2. 10
   3. 18
   4. 24
5. Any part of a scaffold that has been damaged or weakened must be immediately taken out of service and evaluated for repair or replacement in accordance with the manufacturer's requirements.
   1. True
   2. False

| SAFETY MEETING QUIZ |
| --- |
| | ANSWER KEY | | | --- | --- | | Safety Topic: | *V1-109 Fall Protection – Suspended Scaffolds* | |

1. According to OSHA, suspension scaffolds, also known as swing-stage scaffolds, are perhaps the most common type of suspended scaffold.
   1. two-point adjustable
   2. three-point fixed
   3. four-point versatile
   4. five-point stationary
2. Suspension scaffold outrigger beams, cornice hooks, parapet clamps and similar devices must rest of surfaces capable of supporting at least times the load imposed on them by the scaffold, operating at the rated load of the hoist.
   1. 2
   2. 4
   3. 8
   4. 16
3. Items or material that cannot be used as counterweights include
   1. masonry units.
   2. sand or gravel.
   3. roofing felt.
   4. all of the above.
4. The scaffold platform must be at least inches wide but no more than 36 inches wide.
   1. 6
   2. 10
   3. 18
   4. 24
5. Any part of a scaffold that has been damaged or weakened must be immediately taken out of service and evaluated for repair or replacement in accordance with the manufacturer's requirements.
   1. True
   2. False