| SAFETY MEETING QUIZ |
| --- |
|

| Name:  |  | Date: |  |
| --- | --- | --- | --- |
| Safety Topic: | *V1-119 Site Safety – Rebar* |

 |

1. Rebar job site safety hazards include
	1. cuts and pinches.
	2. trips and strains.
	3. puncture and impalement.
	4. all of the above.
2. Place mushroom caps (that are not reinforced with steel) on rebar to prevent cuts, abrasions, and other minor injuries only when there is impalement hazard.
	1. no
	2. potential
	3. minor
	4. significant
3. All protruding reinforcing steel, onto and into which employees could fall, shall be
	1. left unprotected.
	2. surrounded with orange safety cones.
	3. tied with yellow hazard tape as a warning.
	4. guarded to eliminate the hazard of impalement.
4. To prevent injuries on the construction site when working with rebar, use proper lifting techniques and do not carry more than you can handle.
	1. True
	2. False
5. Always wear and eye protection when handling and tying rebar.
	1. a toolbelt
	2. gloves
	3. rubber boots
	4. hearing protection

| SAFETY MEETING QUIZ |
| --- |
|

| ANSWER KEY |
| --- |
| Safety Topic: | *V1-119 Site Safety – Rebar* |

 |

1. Rebar job site safety hazards include
	1. cuts and pinches.
	2. trips and strains.
	3. puncture and impalement.
	4. all of the above.
2. Place mushroom caps (that are not reinforced with steel) on rebar to prevent cuts, abrasions, and other minor injuries only when there is impalement hazard.
	1. no
	2. potential
	3. minor
	4. significant
3. All protruding reinforcing steel, onto and into which employees could fall, shall be
	1. left unprotected.
	2. surrounded with orange safety cones.
	3. tied with yellow hazard tape as a warning.
	4. guarded to eliminate the hazard of impalement.
4. To prevent injuries on the construction site when working with rebar, use proper lifting techniques and do not carry more than you can handle.
	1. True
	2. False
5. Always wear and eye protection when handling and tying rebar.
	1. a toolbelt
	2. gloves
	3. rubber boots
	4. hearing protection