| SAFETY MEETING QUIZ |
| --- |
|

| Name:  |  | Date: |  |
| --- | --- | --- | --- |
| Safety Topic: | *V1-132 Fall Protection – Anchor Points* |

 |

1. An example of a safe anchor point, if installed correctly, is
	1. ductwork or an overhead pipe.
	2. a beam clamp.
	3. any light fixture.
	4. a sturdy ladder.
2. Guardrails and railings can always be used as a safe anchor point.
	1. True
	2. False
3. Anchor points can be
	1. reusable.
	2. permanent.
	3. freestanding.
	4. any of the above.
4. When workers do not require access to the work location on a regular basis, they may use a anchor which will be removed and destroyed after one use.
	1. single-use
	2. vacuum
	3. strap
	4. permanent
5. Before use, a qualified person should evaluate the anchor points with a focus on proper strength.
	1. True
	2. False

| SAFETY MEETING QUIZ |
| --- |
|

| ANSWER KEY |
| --- |
| Safety Topic: | *V1-132 Fall Protection – Anchor Points* |

 |

1. An example of a safe anchor point, if installed correctly, is
	1. ductwork or an overhead pipe.
	2. a beam clamp.
	3. any light fixture.
	4. a sturdy ladder.
2. Guardrails and railings can always be used as a safe anchor point.
	1. True
	2. False
3. Anchor points can be
	1. reusable.
	2. permanent.
	3. freestanding.
	4. any of the above.
4. When workers do not require access to the work location on a regular basis, they may use a anchor which will be removed and destroyed after one use.
	1. single-use
	2. vacuum
	3. strap
	4. permanent
5. Before use, a qualified person should evaluate the anchor points with a focus on proper strength.
	1. True
	2. False