| SAFETY MEETING QUIZ |
| --- |
|

| Name:  |  | Date: |  |
| --- | --- | --- | --- |
| Safety Topic: | *V1-148 Site Safety – Demolition Preparation* |

 |

1. Preparation is key before beginning any demolition work. It is important to plan for
	1. methods that will be used to bring the building down.
	2. fire and collapse prevention.
	3. PPE selection.
	4. all of the above.
2. If it is necessary to maintain any power, water or other utilities during demolition, such lines shall be , as necessary.
	1. turned off
	2. temporarily relocated
	3. demolished
	4. loosened
3. Post signs at each level to warn of the hazard of
	1. dirt and debris.
	2. static electricity.
	3. slippery surfaces.
	4. falling materials.
4. Guard wall openings to a height of
	1. 6 inches.
	2. 2 feet.
	3. 1 meter.
	4. 42 inches.
5. Only those stairways, passageways, and ladders, designated as means of access to the structure of a building, should be used. Other access ways must be entirely closed at all times.
	1. True
	2. False

| SAFETY MEETING QUIZ |
| --- |
|

| ANSWER KEY |
| --- |
| Safety Topic: | *V1-148 Site Safety – Demolition Preparation* |

 |

1. Preparation is key before beginning any demolition work. It is important to plan for
	1. methods that will be used to bring the building down.
	2. fire and collapse prevention.
	3. PPE selection.
	4. all of the above.
2. If it is necessary to maintain any power, water or other utilities during demolition, such lines shall be , as necessary.
	1. turned off
	2. temporarily relocated
	3. demolished
	4. loosened
3. Post signs at each level to warn of the hazard of
	1. dirt and debris.
	2. static electricity.
	3. slippery surfaces.
	4. falling materials.
4. Guard wall openings to a height of
	1. 6 inches.
	2. 2 feet.
	3. 1 meter.
	4. 42 inches.
5. Only those stairways, passageways, and ladders, designated as means of access to the structure of a building, should be used. Other access ways must be entirely closed at all times.
	1. True
	2. False