| SAFETY MEETING QUIZ |
| --- |
| | Name: |  | Date: |  | | --- | --- | --- | --- | | Safety Topic: | *V1-163 Incidents – Struck-by* | | | |

1. Struck-by hazards that workers need to be aware of include
   1. rolling, moving, or sliding materials.
   2. vehicles or heavy equipment.
   3. falling or swinging objects.
   4. all of the above.
2. Workers should be wearing appropriate personal protective equipment (PPE) at the work site when struck-by hazards are present which may include protection.
   1. hearing
   2. head
   3. respiratory
   4. heat
3. If a worker must enter the swing area of heavy equipment for any reason, contact as well as confirmed communication (verbal, hand signal, or radio) with the operator must be established, and the worker should not enter the area until the operator signals that it is safe to do so.
   1. hand
   2. written
   3. eye
   4. group
4. Workers should not be in an active roadway without a flagger or spotter.
   1. True
   2. False
5. Rigging equipment must be inspected and defective rigging equipment must be removed from service.
   1. before use
   2. on the first of every month
   3. if it seems worn
   4. every hour

| SAFETY MEETING QUIZ |
| --- |
| | ANSWER KEY | | | --- | --- | | Safety Topic: | *V1-163 Incidents – Struck-by* | |

1. Struck-by hazards that workers need to be aware of include
   1. rolling, moving, or sliding materials.
   2. vehicles or heavy equipment.
   3. falling or swinging objects.
   4. all of the above.
2. Workers should be wearing appropriate personal protective equipment (PPE) at the work site when struck-by hazards are present which may include protection.
   1. hearing
   2. head
   3. respiratory
   4. heat
3. If a worker must enter the swing area of heavy equipment for any reason, contact as well as confirmed communication (verbal, hand signal, or radio) with the operator must be established, and the worker should not enter the area until the operator signals that it is safe to do so.
   1. hand
   2. written
   3. eye
   4. group
4. Workers should not be in an active roadway without a flagger or spotter.
   1. True
   2. False
5. Rigging equipment must be inspected and defective rigging equipment must be removed from service.
   1. before use
   2. on the first of every month
   3. if it seems worn
   4. every hour