| SAFETY MEETING QUIZ |
| --- |
| | Name: |  | Date: |  | | --- | --- | --- | --- | | Safety Topic: | *V1-46 Site Safety – Housekeeping* | | | |

1. Workers should do their part to help avoid and prevent injuries and incidents by practicing on every job and at every worksite.
   1. good housekeeping
   2. karaoke
   3. knife skills
   4. soccer drills
2. OSHA Standard 1926.25(a) states that during the course of construction, alteration, or repairs, form and scrap lumber with protruding nails, and all other debris, shall be work areas, passageways, and stairs, in and around buildings or other structures.
   1. piled up in
   2. thrown around in
   3. kept cleared from
   4. in neat piles in the middle of
3. Whenever materials are dropped more than to any point lying outside the exterior walls of the building, an enclosed chute of wood, or equivalent material, shall be used.
   1. 5 feet
   2. 20 feet
   3. 3 stories
   4. 100 feet
4. It is not necessary to remove or hammer down nails from scrap lumber and other debris.
   1. True
   2. False
5. During construction separate waste and scrap materials from the immediate work area **to avoid**
   1. getting yelled at.
   2. working overtime.
   3. creating trip and slip hazards.
   4. having to wear PPE.

| SAFETY MEETING QUIZ |
| --- |
| | ANSWER KEY | | | --- | --- | | Safety Topic: | *V1-46 Site Safety – Housekeeping* | |

1. Workers should do their part to help avoid and prevent injuries and incidents by practicing on every job and at every worksite.
   1. good housekeeping
   2. karaoke
   3. knife skills
   4. soccer drills
2. OSHA Standard 1926.25(a) states that during the course of construction, alteration, or repairs, form and scrap lumber with protruding nails, and all other debris, shall be work areas, passageways, and stairs, in and around buildings or other structures.
   1. piled up in
   2. thrown around in
   3. kept cleared from
   4. in neat piles in the middle of
3. Whenever materials are dropped more than to any point lying outside the exterior walls of the building, an enclosed chute of wood, or equivalent material, shall be used.
   1. 5 feet
   2. 20 feet
   3. 3 stories
   4. 100 feet
4. It is not necessary to remove or hammer down nails from scrap lumber and other debris.
   1. True
   2. False
5. During construction separate waste and scrap materials from the immediate work area **to avoid**
   1. getting yelled at.
   2. working overtime.
   3. creating trip and slip hazards.
   4. having to wear PPE.