| SAFETY MEETING QUIZ |
| --- |
| | Name: |  | Date: |  | | --- | --- | --- | --- | | Safety Topic: | *V1-96 Work Zones – Traffic Control Devices* | | | |

1. Channelizing devices, like cones, drums, vertical panels and tubular markers, are used when a change in the traffic pattern is necessary to protect the work zone, which may include guiding traffic
   1. from one lane to another.
   2. into a narrower traveled way.
   3. away from pavement drop-offs.
   4. any of the above.
2. All temporary traffic control signs and devices must be in conformance with the requirements of the MUTCD and State DOT standards.
   1. True
   2. False
3. Traffic control drums are generally used
   1. next to temporary traffic control signs for enhanced visibility.
   2. in situations where they will remain in place for a prolonged period of time.
   3. where space restrictions do not allow more visible devices to be used.
   4. on sidewalks.
4. When multiple advance warning signs are needed, the sign should be the first sign that road users see.
   1. Lane Closed
   2. Detour
   3. Flagger
   4. Road Work Ahead
5. Signs and devices should be properly maintained for
   1. cleanliness.
   2. visibility.
   3. correct positioning.
   4. all of the above.

| SAFETY MEETING QUIZ |
| --- |
| | ANSWER KEY | | | --- | --- | | Safety Topic: | *V1-96 Work Zones – Traffic Control Devices* | |

1. Channelizing devices, like cones, drums, vertical panels and tubular markers, are used when a change in the traffic pattern is necessary to protect the work zone, which may include guiding traffic
   1. from one lane to another.
   2. into a narrower traveled way.
   3. away from pavement drop-offs.
   4. any of the above.
2. All temporary traffic control signs and devices must be in conformance with the requirements of the MUTCD and State DOT standards.
   1. True
   2. False
3. Traffic control drums are generally used
   1. next to temporary traffic control signs for enhanced visibility.
   2. in situations where they will remain in place for a prolonged period of time.
   3. where space restrictions do not allow more visible devices to be used.
   4. on sidewalks.
4. When multiple advance warning signs are needed, the sign should be the first sign that road users see.
   1. Lane Closed
   2. Detour
   3. Flagger
   4. Road Work Ahead
5. Signs and devices should be properly maintained for
   1. cleanliness.
   2. visibility.
   3. correct positioning.
   4. all of the above.