| SAFETY MEETING QUIZ |
| --- |
|

| Name:  |  | Date: |  |
| --- | --- | --- | --- |
| Safety Topic: | *V2-07B Personal Protection – Hand Protection* |

 |

1. If a workplace hazard assessment reveals that employees face potential injury to their hands that cannot be eliminated through engineering and work practice controls, workers must wear appropriate hand protection.
	1. True
	2. False
2. If workers don’t wear gloves as required, they may be at risk for
	1. slips, trips, and falls.
	2. hearing damage.
	3. cuts, lacerations, abrasions, or puncture wounds.
	4. respiratory distress.
3. Gloves should fit
	1. loose.
	2. snug.
	3. stiff.
	4. tight.
4. A factor that may influence the selection of protective gloves may be
	1. size and comfort.
	2. grip requirements.
	3. thermal protection.
	4. any of the above.
5. Gloves contaminated with flammable or combustible materials should not be used while working near
	1. water.
	2. other workers.
	3. fire extinguishers.
	4. an ignition source.

| SAFETY MEETING QUIZ |
| --- |
|

| ANSWER KEY |
| --- |
| Safety Topic: | *V2-07B Personal Protection – Hand Protection* |

 |

1. If a workplace hazard assessment reveals that employees face potential injury to their hands that cannot be eliminated through engineering and work practice controls, workers must wear appropriate hand protection.
	1. True
	2. False
2. If workers don’t wear gloves as required, they may be at risk for
	1. slips, trips, and falls.
	2. hearing damage.
	3. cuts, lacerations, abrasions, or puncture wounds.
	4. respiratory distress.
3. Gloves should fit
	1. loose.
	2. snug.
	3. stiff.
	4. tight.
4. A factor that may influence the selection of protective gloves may be
	1. size and comfort.
	2. grip requirements.
	3. thermal protection.
	4. any of the above.
5. Gloves contaminated with flammable or combustible materials should not be used while working near
	1. water.
	2. other workers.
	3. fire extinguishers.
	4. an ignition source.