| SAFETY MEETING QUIZ |
| --- |
|

| Name:  |  | Date: |  |
| --- | --- | --- | --- |
| Safety Topic: | *V2-113 Fall Protection – Fall Arrest Systems* |

 |

1. A personal fall arrest system must be rigged so that a worker can neither free fall more than nor contact any lower level.
	1. 2 feet
	2. 6 feet
	3. 10 feet
	4. 25 feet
2. A personal fall arrest system must be inspected
	1. before each use.
	2. once a week.
	3. every month or so.
	4. annually.
3. A full-body harness should include a on the back for attaching a lifeline or a lanyard.
	1. carabiner
	2. hook
	3. lock
	4. D-ring
4. Lanyards must have a minimum breaking strength of pounds.
	1. 50
	2. 500
	3. 5,000
	4. 50,000
5. PFAS equipment should be stored in a clean, dry area, that is free of fumes, sunlight, corrosive materials, sharp edges, or vibration.
	1. True
	2. False

| SAFETY MEETING QUIZ |
| --- |
|

| ANSWER KEY |
| --- |
| Safety Topic: | *V2-113 Fall Protection – Fall Arrest Systems* |

 |

1. A personal fall arrest system must be rigged so that a worker can neither free fall more than nor contact any lower level.
	1. 2 feet
	2. 6 feet
	3. 10 feet
	4. 25 feet
2. A personal fall arrest system must be inspected
	1. before each use.
	2. once a week.
	3. every month or so.
	4. annually.
3. A full-body harness should include a on the back for attaching a lifeline or a lanyard.
	1. carabiner
	2. hook
	3. lock
	4. D-ring
4. Lanyards must have a minimum breaking strength of pounds.
	1. 50
	2. 500
	3. 5,000
	4. 50,000
5. PFAS equipment should be stored in a clean, dry area, that is free of fumes, sunlight, corrosive materials, sharp edges, or vibration.
	1. True
	2. False