| SAFETY MEETING QUIZ |
| --- |
| | Name: |  | Date: |  | | --- | --- | --- | --- | | Safety Topic: | *V2-113 Fall Protection – Fall Arrest Systems* | | | |

1. A personal fall arrest system must be rigged so that a worker can neither free fall more than nor contact any lower level.
   1. 2 feet
   2. 6 feet
   3. 10 feet
   4. 25 feet
2. A personal fall arrest system must be inspected
   1. before each use.
   2. once a week.
   3. every month or so.
   4. annually.
3. A full-body harness should include a on the back for attaching a lifeline or a lanyard.
   1. carabiner
   2. hook
   3. lock
   4. D-ring
4. Lanyards must have a minimum breaking strength of pounds.
   1. 50
   2. 500
   3. 5,000
   4. 50,000
5. PFAS equipment should be stored in a clean, dry area, that is free of fumes, sunlight, corrosive materials, sharp edges, or vibration.
   1. True
   2. False

| SAFETY MEETING QUIZ |
| --- |
| | ANSWER KEY | | | --- | --- | | Safety Topic: | *V2-113 Fall Protection – Fall Arrest Systems* | |

1. A personal fall arrest system must be rigged so that a worker can neither free fall more than nor contact any lower level.
   1. 2 feet
   2. 6 feet
   3. 10 feet
   4. 25 feet
2. A personal fall arrest system must be inspected
   1. before each use.
   2. once a week.
   3. every month or so.
   4. annually.
3. A full-body harness should include a on the back for attaching a lifeline or a lanyard.
   1. carabiner
   2. hook
   3. lock
   4. D-ring
4. Lanyards must have a minimum breaking strength of pounds.
   1. 50
   2. 500
   3. 5,000
   4. 50,000
5. PFAS equipment should be stored in a clean, dry area, that is free of fumes, sunlight, corrosive materials, sharp edges, or vibration.
   1. True
   2. False