| SAFETY MEETING QUIZ |
| --- |
| | Name: |  | Date: |  | | --- | --- | --- | --- | | Safety Topic: | *V2-142 Ladder Safety – Portable Ladders* | | | |

1. Always inspect every portable ladder
   1. before using it.
   2. at the end of every work shift.
   3. once a month.
   4. annually.
2. When it is necessary to set up a ladder in an area like a , the ladder should be secured, and the area should be barricaded to keep traffic and pedestrians away from the ladder to avoid displacement.
   1. passageway
   2. doorway
   3. driveway
   4. all of the above
3. Maintain good in the areas near ladder use.
   1. toolboxes
   2. attitudes
   3. housekeeping
   4. luck
4. Use your best judgement, sometimes it is safe to stand on the top step (top cap) of a stepladder or on the top three rungs of an extension ladder.
   1. True
   2. False
5. When climbing up and down a ladder workers must face the ladder, use at least one hand to grasp the ladder, and maintain 3-point contact.
   1. True
   2. False

| SAFETY MEETING QUIZ |
| --- |
| | ANSWER KEY | | | --- | --- | | Safety Topic: | *V2-142 Ladder Safety – Portable Ladders* | |

1. Always inspect every portable ladder
   1. before using it.
   2. at the end of every work shift.
   3. once a month.
   4. annually.
2. When it is necessary to set up a ladder in an area like a , the ladder should be secured, and the area should be barricaded to keep traffic and pedestrians away from the ladder to avoid displacement.
   1. passageway
   2. doorway
   3. driveway
   4. all of the above
3. Maintain good in the areas near ladder use.
   1. toolboxes
   2. attitudes
   3. housekeeping
   4. luck
4. Use your best judgement, sometimes it is safe to stand on the top step (top cap) of a stepladder or on the top three rungs of an extension ladder.
   1. True
   2. False
5. When climbing up and down a ladder workers must face the ladder, use at least one hand to grasp the ladder, and maintain 3-point contact.
   1. True
   2. False