| SAFETY MEETING QUIZ |
| --- |
| | Name: |  | Date: |  | | --- | --- | --- | --- | | Safety Topic: | *V2-48 Materials Handling – Pallet Jacks* | | | |

1. Pallet jacks are commonly regarded as being safer than a forklift, but there are still safety hazards that all pallet jack operators should be aware of.
   1. True
   2. False
2. A common hazard associated with pallet jacks is
   1. foot injury, when loads are dropped or the pallet jack moves over a worker’s foot.
   2. back trauma, from moving a loaded pallet jack or adjusting a heavy load.
   3. property damage, when the heavy load strikes a corner, column, wall or other stationary object.
   4. all of the above.
3. When operating a pallet jack **never**
   1. ensure the loads are evenly stacked on the forks.
   2. allow someone to ride on the forks.
   3. wear required PPE.
   4. keep loads close to the ground.
4. When operating a pallet jack **always**
   1. know the maximum load limit and do not overload.
   2. start moving fast and come to a stop quickly.
   3. steer onto uneven surfaces and steep inclines.
   4. remove the warning stickers.
5. When not in use, pallet jacks should be rolled into an area that
   1. blocks emergency exits.
   2. is on an incline.
   3. does not have pedestrian traffic.
   4. is in front of fire extinguishers.

| SAFETY MEETING QUIZ |
| --- |
| | ANSWER KEY | | | --- | --- | | Safety Topic: | *V2-48 Materials Handling – Pallet Jacks* | |

1. Pallet jacks are commonly regarded as being safer than a forklift, but there are still safety hazards that all pallet jack operators should be aware of.
   1. True
   2. False
2. A common hazard associated with pallet jacks is
   1. foot injury, when loads are dropped or the pallet jack moves over a worker’s foot.
   2. back trauma, from moving a loaded pallet jack or adjusting a heavy load.
   3. property damage, when the heavy load strikes a corner, column, wall or other stationary object.
   4. all of the above.
3. When operating a pallet jack **never**
   1. ensure the loads are evenly stacked on the forks.
   2. allow someone to ride on the forks.
   3. wear required PPE.
   4. keep loads close to the ground.
4. When operating a pallet jack **always**
   1. know the maximum load limit and do not overload.
   2. start moving fast and come to a stop quickly.
   3. steer onto uneven surfaces and steep inclines.
   4. remove the warning stickers.
5. When not in use, pallet jacks should be rolled into an area that
   1. blocks emergency exits.
   2. is on an incline.
   3. does not have pedestrian traffic.
   4. is in front of fire extinguishers.