| SAFETY MEETING QUIZ |
| --- |
|

| Name:  |  | Date: |  |
| --- | --- | --- | --- |
| Safety Topic: | *V1-106 Driving Safety – Winter Driving on Site* |

 |

1. Check vehicles to ensure that equipment is in safe operating condition.
	1. at the beginning of each shift
	2. every 30 minutes
	3. at night
	4. once a month
2. Ensure on heavy equipment, trucks and work vehicles are kept clean and clear.
	1. windows
	2. mirrors
	3. lights
	4. all of the above
3. During winter, all workers should be wearing
	1. rubber boots.
	2. high-visibility safety gear.
	3. a whistle.
	4. two pairs of gloves.
4. Ensure all driving moves in wintery weather are to avoid spinning or skidding.
	1. sudden and abrupt
	2. gentle and gradual
	3. swift and snappy
	4. careless and sloppy
5. When driving on hills, pick a path that provides
	1. high momentum.
	2. a slippery slope.
	3. the most traction.
	4. unseen hazards.

| SAFETY MEETING QUIZ |
| --- |
|

| ANSWER KEY |
| --- |
| Safety Topic: | *V1-106 Driving Safety – Winter Driving on Site* |

 |

1. Check vehicles to ensure that equipment is in safe operating condition.
	1. at the beginning of each shift
	2. every 30 minutes
	3. at night
	4. once a month
2. Ensure on heavy equipment, trucks and work vehicles are kept clean and clear.
	1. windows
	2. mirrors
	3. lights
	4. all of the above
3. During winter, all workers should be wearing
	1. rubber boots.
	2. high-visibility safety gear.
	3. a whistle.
	4. two pairs of gloves.
4. Ensure all driving moves in wintery weather are to avoid spinning or skidding.
	1. sudden and abrupt
	2. gentle and gradual
	3. swift and snappy
	4. careless and sloppy
5. When driving on hills, pick a path that provides
	1. high momentum.
	2. a slippery slope.
	3. the most traction.
	4. unseen hazards.