| SAFETY MEETING QUIZ |
| --- |
| | Name: |  | Date: |  | | --- | --- | --- | --- | | Safety Topic: | *V1-32B Man Lifts – Scissor Lifts* | | | |

1. Scissor lifts can pose serious risks to workers if they are not operated properly and safely.
   1. True
   2. False
2. Never the rated load capacity of the scissor lift as provided by the manufacturer.
   1. surrender
   2. exceed
   3. repeat
   4. write
3. When stability is required, use
   1. inspections.
   2. ladders.
   3. hard hats.
   4. outriggers.
4. Avoid operating scissor lifts in
   1. high winds.
   2. warehouses.
   3. sunny weather.
   4. parking lots.
5. Never the guardrail components of a scissor lift.
   1. stand on
   2. step up on
   3. step over
   4. any of the above

| SAFETY MEETING QUIZ |
| --- |
| | ANSWER KEY | | | --- | --- | | Safety Topic: | *V1-32B Man Lifts – Scissor Lifts* | |

1. Scissor lifts can pose serious risks to workers if they are not operated properly and safely.
   1. True
   2. False
2. Never the rated load capacity of the scissor lift as provided by the manufacturer.
   1. surrender
   2. exceed
   3. repeat
   4. write
3. When stability is required, use
   1. inspections.
   2. ladders.
   3. hard hats.
   4. outriggers.
4. Avoid operating scissor lifts in
   1. high winds.
   2. warehouses.
   3. sunny weather.
   4. parking lots.
5. Never the guardrail components of a scissor lift.
   1. stand on
   2. step up on
   3. step over
   4. any of the above