| SAFETY MEETING QUIZ |
| --- |
|

| Name:  |  | Date: |  |
| --- | --- | --- | --- |
| Safety Topic: | *V1-57 Tool Safety – Welding and Cutting* |

 |

1. Specific precautions must be taken during high-hazard work, like welding and cutting, to prevent personal injury and workplace damage.
	1. True
	2. False
2. All employees working in a hot work area should know where are located.
	1. the fire exits
	2. firefighting equipment
	3. the fire alarms
	4. all of the above
3. In welding environments clothing is recommended.
	1. vinyl
	2. leather and flame-resistant treated cotton
	3. normal
	4. expensive
4. Welding activities must be performed in an area that is free from
	1. firefighting equipment.
	2. adequate ventilation.
	3. flammable materials.
	4. sufficient PPE.
5. Wear if working in an area with high noise levels.
	1. hearing protection
	2. a hard hat
	3. a shop apron
	4. steel-toed boots

| SAFETY MEETING QUIZ |
| --- |
|

| ANSWER KEY |
| --- |
| Safety Topic: | *V1-57 Tool Safety – Welding and Cutting* |

 |

1. Specific precautions must be taken during high-hazard work, like welding and cutting, to prevent personal injury and workplace damage.
	1. True
	2. False
2. All employees working in a hot work area should know where are located.
	1. the fire exits
	2. firefighting equipment
	3. the fire alarms
	4. all of the above
3. In welding environments clothing is recommended.
	1. vinyl
	2. leather and flame-resistant treated cotton
	3. normal
	4. expensive
4. Welding activities must be performed in an area that is free from
	1. firefighting equipment.
	2. adequate ventilation.
	3. flammable materials.
	4. sufficient PPE.
5. Wear if working in an area with high noise levels.
	1. hearing protection
	2. a hard hat
	3. a shop apron
	4. steel-toed boots