| SAFETY MEETING QUIZ |
| --- |
|

| Name:  |  | Date: |  |
| --- | --- | --- | --- |
| Safety Topic: | *V1-98 Work Zones – High-Visibility Safety Apparel* |

 |

1. Class 1 Type O high-visibility safety apparel is suitable for
	1. off-road and non-roadway use.
	2. roadway work.
	3. temporary traffic control zones.
	4. law enforcement personnel.
2. All workers who are exposed to traffic or work vehicles and construction equipment within the temporary traffic control zone must wear high-visibility safety apparel that
	1. is fluorescent orange.
	2. is Class 1 Type O.
	3. has long sleeves.
	4. meets the Performance Class 2 or 3 requirements.
3. Performance provides the highest level of visibility provided by a HVSA garment.
	1. Class 1
	2. Class 2
	3. Class 3
	4. Class 4
4. A safety vest without sleeves can be rated for Class 2 or Class 3 protection.
	1. True
	2. False
5. Most HVSA that is worn on a daily basis will last approximately
	1. 1 week.
	2. 30 days.
	3. 6 months.
	4. 3 years.

| SAFETY MEETING QUIZ |
| --- |
|

| ANSWER KEY |
| --- |
| Safety Topic: | *V1-98 Work Zones – High-Visibility Safety Apparel* |

 |

1. Class 1 Type O high-visibility safety apparel is suitable for
	1. off-road and non-roadway use.
	2. roadway work.
	3. temporary traffic control zones.
	4. law enforcement personnel.
2. All workers who are exposed to traffic or work vehicles and construction equipment within the temporary traffic control zone must wear high-visibility safety apparel that
	1. is fluorescent orange.
	2. is Class 1 Type O.
	3. has long sleeves.
	4. meets the Performance Class 2 or 3 requirements.
3. Performance provides the highest level of visibility provided by a HVSA garment.
	1. Class 1
	2. Class 2
	3. Class 3
	4. Class 4
4. A safety vest without sleeves can be rated for Class 2 or Class 3 protection.
	1. True
	2. False
5. Most HVSA that is worn on a daily basis will last approximately
	1. 1 week.
	2. 30 days.
	3. 6 months.
	4. 3 years.