| SAFETY MEETING QUIZ |
| --- |
|

| Name:  |  | Date: |  |
| --- | --- | --- | --- |
| Safety Topic: | *V2-06B Personal Protection – Foot Protection* |

 |

1. OSHA requires that adequate foot protection be used whenever the work conditions pose hazards that could cause a foot injury.
	1. True
	2. False
2. When determining footwear requirements, many factors should be considered during the hazard assessment process, including
	1. the tasks being performed.
	2. environmental conditions.
	3. electrical hazards.
	4. all of the above.
3. A -resistant sole may be required when a working environment may potentially have sharp objects like nails or broken glass.
	1. water
	2. puncture
	3. heat
	4. chemical
4. A guard may be required when additional protection is needed for the top of the foot.
	1. metatarsal
	2. insulated
	3. ESD
	4. waterproof
5. Shoes and boots should be replaced when the tread pattern is gone from the rear two-thirds of the heel.
	1. True
	2. False

| SAFETY MEETING QUIZ |
| --- |
|

| ANSWER KEY |
| --- |
| Safety Topic: | *V2-06B Personal Protection – Foot Protection* |

 |

1. OSHA requires that adequate foot protection be used whenever the work conditions pose hazards that could cause a foot injury.
	1. True
	2. False
2. When determining footwear requirements, many factors should be considered during the hazard assessment process, including
	1. the tasks being performed.
	2. environmental conditions.
	3. electrical hazards.
	4. all of the above.
3. A -resistant sole may be required when a working environment may potentially have sharp objects like nails or broken glass.
	1. water
	2. puncture
	3. heat
	4. chemical
4. A guard may be required when additional protection is needed for the top of the foot.
	1. metatarsal
	2. insulated
	3. ESD
	4. waterproof
5. Shoes and boots should be replaced when the tread pattern is gone from the rear two-thirds of the heel.
	1. True
	2. False