| SAFETY MEETING QUIZ |
| --- |
| | Name: |  | Date: |  | | --- | --- | --- | --- | | Safety Topic: | *V2-43 Incidents – Caught-in* | | | |

1. Caught-in Hazards are one of the Top 4 areas of workplace fatalities.
   1. True
   2. False
2. To avoid caught-in hazards on the job, **always**
   1. inspect machinery and equipment prior to operation.
   2. ensure that warning alarms and horns are working properly every day.
   3. maintain safe distances from potential hazards.
   4. all of the above.
3. Never attempt to operate equipment unless you have been
   1. yelled at.
   2. trained and authorized.
   3. told by someone else.
   4. working late.
4. To avoid caught-in hazards, **never**
   1. crawl or enter potentially unstable areas.
   2. take a bathroom break.
   3. listen to your supervisor.
   4. finish your lunch.
5. Training in proper is needed before performing repair, service or maintenance activities on equipment.
   1. housekeeping
   2. bucket trucks
   3. fall protection
   4. lockout and tagout procedures

| SAFETY MEETING QUIZ |
| --- |
| | ANSWER KEY | | | --- | --- | | Safety Topic: | *V2-43 Incidents – Caught-in* | |

1. Caught-in Hazards are one of the Top 4 areas of fatalities in construction.
   1. True
   2. False
2. To avoid caught-in hazards on the job, **always**
   1. inspect machinery and equipment prior to operation.
   2. ensure that warning alarms and horns are working properly every day.
   3. maintain safe distances from potential hazards.
   4. all of the above.
3. Never attempt to operate equipment unless you have been
   1. yelled at.
   2. trained and authorized.
   3. told by someone else.
   4. working late.
4. To avoid caught-in hazards, **never**
   1. crawl or enter potentially unstable areas.
   2. take a bathroom break.
   3. listen to your supervisor.
   4. finish your lunch.
5. Training in proper is needed before performing repair, service or maintenance activities on equipment.
   1. housekeeping
   2. bucket trucks
   3. fall protection
   4. lockout and tagout procedures