| SAFETY MEETING QUIZ |
| --- |
| | Name: |  | Date: |  | | --- | --- | --- | --- | | Safety Topic: | *V2-95 Electrical Safety – Arc Flash* | | | |

1. An arc flash is an energy discharge of that forms when a fault occurs in an electrical circuit.
   1. repetitive vibration
   2. light and heat
   3. biological hazards
   4. chemical exposure
2. An arc flash can cause
   1. blindness or hearing loss.
   2. minor injuries or nerve damage.
   3. cardiac arrest.
   4. any of the above.
3. When possible, perform work on de-energized equipment and always use procedures.
   1. administrative
   2. occupational
   3. substitution
   4. lockout/tagout
4. Deadly burns can occur even when a worker is several feet away from an arc flash.
   1. True
   2. False
5. Only employees are allowed to work on equipment that has not been shut off and locked/tagged.
   1. equipped
   2. cautious
   3. qualified
   4. prepared

| SAFETY MEETING QUIZ |
| --- |
| | ANSWER KEY | | | --- | --- | | Safety Topic: | *V2-95 Electrical Safety – Arc Flash* | |

1. An arc flash is an energy discharge of that forms when a fault occurs in an electrical circuit.
   1. repetitive vibration
   2. light and heat
   3. biological hazards
   4. chemical exposure
2. An arc flash can cause
   1. blindness or hearing loss.
   2. minor injuries or nerve damage.
   3. cardiac arrest.
   4. any of the above.
3. When possible, perform work on de-energized equipment and always use procedures.
   1. administrative
   2. occupational
   3. substitution
   4. lockout/tagout
4. Deadly burns can occur even when a worker is several feet away from an arc flash.
   1. True
   2. False
5. Only employees are allowed to work on equipment that has not been shut off and locked/tagged.
   1. equipped
   2. cautious
   3. qualified
   4. prepared